{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Antenna isolation calculator"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Antenna isolation calculator","index":0,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[[4,1,5,1],[4,2,5,2],[6,1,7,1],[6,2,7,2]],"flags":["formulas_cached_only"]}
["Antenna isolation calculator"]
[]
["   Usage: Enter frequency and isolation to calculate separation."]
[]
["Ant. 1 radiation pattern attenuation","dB",15]
["(towards antenna 2, 15 dB for dipoles)"]
["Ant. 2 radiation pattern attenuation","dB",15]
["(towards antenna 1, 15 dB for dipoles)"]
["Frequency","MHz",100]
["Isolation","dB",65]
["Separation","m",13.424910241333654]
[]
["   Default separation is valid for vertically polarized yagi and"]
["   dipole based antennas installed on the same vertical axis."]