{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":14,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Quantity","Unit","Value","Description"]
["dl","km",10,"link distance"]
["fo","MHz",450,"operating frequency"]
["htx","m",10,"tx antenna height above ground"]
["hrx","m",10,"rx antenna height above ground"]
["Lp","dB",141.1626070182482,"propagation Loss"]
[]
["Ptx","dBm",30,"tx output Power"]
["Ltx","dB",2,"tx feedline Loss"]
["Gtx","dBi",12,"tx antenna Gain"]
["Lp","dB",141.1626070182482,"propagation Loss"]
["Grx","dBi",12,"rx antenna Gain"]
["Lrx","dB",2,"rx feedline Loss"]
["Prx","dBm",-91.1626070182482,"rx input Power"]
[]
["Srx","dBm",-112,"rx Sensitivity"]
["FM","dB",20.837392981751805,"Fade Margin"]